**Annual Auditing of**

**Pre-qualification requirement of DI Pipes and Fittings**

**Current Details Previous Details**

**Benxi Beitai Ductile Cast Iron Pipes Co., Ltd.**

, Betai Town, Pingshan District, Benxi City, Liaoning Province, P.R.China.

**Yingkou Economic & Technology Development Zone Xinfeng Pipe Fitting Co., Ltd.**

Jintun Village, Hongqi Town, Bayuquan District, Liaoning Province, P R China.

**Savinda Enterprises (Pvt) Ltd.,** 176 F, Saranatissa Mawatha, Kahathuduwa, Polgasowita.

**Yingkou Jiahua Plastic New Technology Co., Ltd.**

BA YU Quan, Yingkou City,

Bayujuan Area Plastic Industrial Park(01-The red Se Xinxin Rubber Factory)

P R China.

**Benxi Beitai Ductile Cast Iron Pipes Co. Ltd.**

Betai Town, , Benxi City, Liaoning Province, P.R.China.

**Pipe Manufacturer :Benxi Beitai Ductile Cast Iron Pipes Co., Ltd.** Beitai Town,

Pingshan District, Benxi City, Liaoning Province

**Fitting Manufacturer :Yingkou Economic and Technology Development Zone**

**XingFeng Pipe Fittings Co., Ltd.**, Jintun Village, Hongqi

Town, Liaonan Street, Bayuquan District, Yingkou City,

Liaoning, P.R. China.

**Local Agent : SavindaEnterprises (Pvt.) Ltd.** 176 F, Saranatissa

Mawatha, Kahathuduwa, Polgasowita.

**Rubber Ring :** **Yingkou Jiahua Plastic new Technology Co., Ltd.,**

Yingkou City Bayujuan Area Plastic Industrial Park (01-

the red sea Xinxin Rubber Factory), P.R. China

**Restrained pipes : Benxi Beitai Ductile Cast Iron Pipes Co. Ltd.**

Betai Town, , Benxi City, Liaoning Province, P.R.China.

| **No** | **Description of the Requirement** | **Yes/No** | **Validity period** | **Details/**  **Description** | **Remarks** |
| --- | --- | --- | --- | --- | --- |
| **2** | **Technical details required** |  |  |  |  |
| (a) | Valid ISO 9001:2015 Quality Management System Certificate in operation from an accredited agency which is a member of International Accreditation Forum (IAF).  *The certifications should indicate the applicability for pipes and fittings, factory locations, product range and validity. The certificates shall be for the particular factory and for the particular range of products.* | Pipe: | 20.05.2020 – 19.05.2023 | Name: **Benxi Beitai Ductile Cast Iron Pipes Co., Ltd.**  Certificate No:  02220Q3023R4L  GHC | Certificate is ok.  But the name was different. Please verify the name. (The certificate and its verification attached herewith as Annex 2A) |
| Fitting: | 24.08.2021 –  23.08.2024 | Name: **Yingkou Economic and Technology Development Zone XingFeng Pipe Fittings Co., Ltd.**,  Certificate No  CN-00221Q25344R0S  Diameter range: DN 80mm-2600mm  QNet | **Accepted** |
| (b) | Valid product conformity certificate conforming to BSEN 545:2010 / ISO 2531:2009 / BSEN 598:2007+A1:2009 / ISO 7186:2011 for **DI pipes & fittings**; issued by an Accredited Agency which is a member of International Accreditation Forum (IAF) | Pipe: | Valid until 27.06.2022 | Name: **Benxi Beitai Ductile Cast Iron Pipes Co., Ltd.**  Certificate No:  IN-DL-5805-21051-TC  Diameter range: DN 80 – 2600mm  SGS | **Accepted** |
| Fitting: | Valid to 21.06.2022 | Name: **Yingkou Economic and Technology Development Zone XingFeng Pipe Fittings Co., Ltd.**,  Certificate No:  IN-DL-5805-21050-C  Dia.range:DN80-2600mm  SGS | **Accepted** |
| (c) | Valid **ISO 9001:2015** Quality Management System Certificate for **Rubber rings** and **Nuts & Bolts**, which shall be manufactured to conform to the **specifications** |  | Valid until 14.04.2023 | Name: **Yingkou Jiahua Plastic new Technology Co., Ltd.,**  Certificate No:  02420Q31010395R2S  Diameter range:  Universal certification centre | **Accepted** |
| (d) | Valid product conformity certificate conforming to BSEN 681-1:1996 / ISO 4633:2015 for **Rubber rings**; issued by an Accredited Agency which is a member of International Accreditation Forum (IAF) |  | Valid until 02.08.2022 | Name: **Yingkou Jiahua Plastic new Technology Co., Ltd.,**  Certificate No:  IN-DL-5805-21061  Diameter range:  SGS | **Accepted** |
| (e) | For self-anchoring (restrained) joints, a Type Test Certificate issued by an Accredited Inspection Agency which is a member of International Accredited Forum (IAF) and evidence of previous supplies shall be provided (ISO 10804:2010). |  | Valid to 19.11.2021 | Name: **Benxi Beitai Ductile Cast Iron Pipes Co., Ltd.**  Certificate No:  IN-DL-5805-20038-C  Diameter range:  DN 80-2600mm  SGS | **Expired**  Letter has given and informed the certificate is in renewing progress.  Shall Submit the valid certificate |